## PCAE

### Notes

- The resistors connected to the parallel port (drawn horizontally) are 1k Ohm
  The resistors connected to pin 1 of the joystick port (drawn vertically) are 4.7k Ohm
- It is not recommended to build this interface. Rather build Amiga4Player.
- This interface is not currently supported by PPJoy
- General notes about interface construction

### Credits

The original diagram and information for this interface can be found at http://www.classicgaming.com/pcae/.
Back to PPJoy interface diagrams.