## DirectPad Pro PSX interface

Controller | Parallel Port
--- | ---
Pad 1 | Pad 2
1 (Dat) | 10 | 13
2 (Cmd) | 2
3 (+7v) | +7.6v
4 (Gnd) | 18
5 (+3v) | +3.5v
6 (Sel) | 3
7 (Clk) | 4
8 | -
9 (Ack) | 12 | 15

### Notes

- This is the interface that DirectPad Pro used when "Multitap" is set to off. When "Multitap" is selected, DirectPad Pro uses the Megatap interface.
- See the Powering PSX pads page for details on how to provide the +3.5v and +7.6v required by the PSX pads.
- General notes about interface construction

### Credits

The original diagram and information for this interface can be found at http://www.arcadecontrols.com/Mirrors/www.ziplabel.com/dpadpro/psx.html.
Back to PPJoy interface diagrams.