## NTPad XP interface

Controller | Parallel Port
--- | ---
Pad 1 | Pad 2 | Pad 3 | Pad 4 | Pad 5
1 (Dat) | 10
2 (Cmd) | 2
3 (+7v) | +7.6v
4 (Gnd) | 18
5 (+3v) | +3.5v
6 (Sel) | 3
7 (Clk) | 4 | 5 | 6 | 7 | 8
8 | -
9 (Ack) | 12

### Notes

- The pin numbering for the PSX connector presented here is reversed from the numbering on the NTPad XP web page. Also the original web page shows the connector looking into the CONNECTOR ON THE CONSOLE.
- See the Powering PSX pads page for details on how to provide the +3.5v and +7.6v required by the PSX pads.
- General notes about interface construction

### Credits

The original diagram and information for this interface can be found at http://www.ntpad.com.ar/.
Back to PPJoy interface diagrams.